**INTERIM LIFE SAFETY MEASURE IMPLEMENTATION DOCUMENTATION**

 **Project Name/Number:** Click here to enter text. **Project Location:** Click here to enter text.

 **Start Date:** Click here to enter a date. **Projected Completion Date:** Click here to enter a date.

| **Required****Yes/No** | **Required Action** | **Implementation Plan** | **Problems, failures, user errors****Corrective actions** |
| --- | --- | --- | --- |
|  | Notify fire department when a fire alarm or sprinkler systems is out of service more than 4 hours in a 24-hour period in an occupied building. Notification and fire watch times are documented. | System and date/time out of service:Date fire department notified:Notified by:Documentation attached |  |
|  | Initiate a fire watch initiated when a fire alarm or sprinkler systems is out of service more than 4 hours in a 24-hour period in an occupied building. Notification and fire watch times are documented. | System and date/time out of service:Date/time initiated:Notified by:Documentation attached |  |
|  | Post signage to identify the location of alternate exits to everyone affected.  | Signage posted at following locations: |  |
| Additional steps taken when LSC deficiencies cannot be immediately corrected or during periods of construction: |
|  | Inspect exits in affected areas on a daily basis.  | Exits requiring inspections:Persons assigned to carry out inspections:Date assigned persons trained: |  |
|  | Provide temporary but equivalent fire alarm and detection systems provided when a fire system is impaired.  | Type fire alarm/detection system provided and locations: |  |
|  | Provide additional fire-fighting equipment. | Additional fire-fighting equipment provided and locations: |  |
|  | Use temporary construction partitions that are smoke-tight, or made of noncombustible material or made of limited-combustible materials that will not contribute to the development or spread of fire.  | Temporary construction partitions located at: |  |
|  | Increase surveillance of buildings, grounds, and equipment, giving special attention to construction areas and storage, excavation, and field offices.  | Areas requiring inspection:Persons assigned to carryout inspections:Date assigned persons trained: |   |
|  | Enforce storage, housekeeping, and debris-removal practices that reduce the building’s flammable and combustible fire load to the lowest feasible level.  | Areas requiring inspection:Persons assigned to carryout inspections:Date assigned persons trained: |  |
|  | Provide additional training to staff on the use of fire-fighting equipment.  | Departments/services requiring training:Training method: Training completed:Training roster attached |   |
|  | Conduct one additional fire drill per shift per quarter.  | Departments/services requiring additional fire drills:Documentation attached |  |
|  | Inspect and test temporary systems monthly. The completion date of the tests is documented.  | Temporary systems requiring inspections/tests:Documentation attached |  |
|  | Educate staff to promote awareness of building deficiencies, construction hazards, and temporary measures implemented to maintain fire safety.  | Departments/services requiring training:Training method: Training completed:Training roster attached |  |
|  | Train staff on impaired structural or compartmental fire safety features that prevent the spread of fire and products of combustion to provide a safe means of egress to an approved exit. Compartmentalization includes building components such as fire-rated walls and doors, smoke barriers, and fire-rated floor slabs.  | Departments/services requiring training:Training method: Training completed:Training roster attached |  |