FIRE SAFETY INSPECTION CHECKLIST

**CONSTRUCTION, ALTERATION AND DEMOLITION OPERATIONS**

|  |  |
| --- | --- |
| **Project No:** Click here to enter text. | **Inspector:** Click here to enter text. |
| **Location:** Click here to enter text. | **Date of Inspection:** Click here to enter a date. |
| **Requirement** | **Yes** | **No** | **N/A** |
| **MEANS OF EGRESS** | Building exits provide free and unobstructed egress. |  |  |  |
| Adequate escape facilities are present and unobstructed for use by construction workers. |  |  |  |
| There is no evidence of storage in stairwells.  |  |  |  |
| Stairwell doors are unblocked and maintained in the closed position. |  |  |  |
| **FIRE PROTECTION** | Fire alarm, detection and suppression systems are operational. Affected systems are noted in remarks. |  |  |  |
| Fire Department access to hydrants, standpipes, etc. is unobstructed. |  |  |  |
| Construction partitions are non-combustible and smoke-tight. |  |  |  |
| Cutting, burning, or welding is performed by permit only. |  |  |  |
| Fire extinguishers are sufficient in number and of the appropriate type. |  |  |  |
| Flammable liquids are limited in quantity, used, and stored properly. |  |  |  |
| Bulk quantities of flammable liquids/gases are stored outside of the construction area. |  |  |  |
| Where applicable, smoke barrier and fire barrier doors are unobstructed and functioning properly. |  |  |  |
| **ELEC-TRICAL** | Temporary wiring is properly protected, grounded, and supported. |  |  |  |
| There is no evidence of unprotected splices. |  |  |  |
| **HOUSE-KEEPING** | Temporary lighting is equipped with guards or at sufficient height to prevent accidental contact. |  |  |  |
| Quantities of combustible materials are stored externally until needed. |  |  |  |
| Combustible debris is removed daily or more frequently when required. |  |  |  |
| **GENERAL** | Access to emergency services is unaffected by construction. |  |  |  |
| Access to construction area is limited to authorize personnel only. Security measures are in place and adequate. |  |  |  |
| Smoking is not permitted in or adjacent to the construction area. |  |  |  |
| Floor openings, platforms, etc. are properly guarded. |  |  |  |
| Excavations are properly sloped or shored. |  |  |  |
| Excavations are properly guarded by appropriate fencing, barricades etc. |  |  |  |
| Temporary heating equipment is used in accordance with manufacturer’s recommendations. |  |  |  |
| **REMARKS:** |

**Inspector’s Signature**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Title**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Reviewed April 2015