**INTERIM LIFE SAFETY MEASURES SELECTION MATRIX**

|  |  |
| --- | --- |
| **EXISTING SIGNIFICANT LIFE SAFETY CODE DEFICIENCIES OR****CONDITIONS AS A RESULT OF CONSTRUCTION** | **INTERIM LIFE SAFETY MEASURE** |
| Inspect exits daily | Temporary fire alarm and detection system | Additional firefighting equipment | Temporary construction partitions | Increased surveillance | Enforce storage, housekeeping and debris removal practices | Additional training on the use of firefighting equipment | Additional fire drill per shift per quarter | Inspect and test temporary systems monthly | Staff awareness training | Additional staff training to on building deficiencies | Notify fire department  | Initiate fire watch  | Post alternative exit signage |
| **Code Deficiencies** | Patient room door latching problem |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Lacking a code complying smoke barrier |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Fire exit stairs discharge improperly |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Excessive travel distance to an approved exit |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Lack of two remote exits |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Nonconforming building construction type  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Improperly protected vertical openings |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Large penetrations in fire barriers |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Corridor walls do not extend to the structure |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Hazardous areas not properly protected |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Construction** | Blocking off an approved exit |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Rerouting of traffic to emergency room |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Major renovation of an occupied floor |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Replacing fire alarm system (out of service) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Installing sprinkler system (out of service) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Significantly modifying smoke or fire barrier walls |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Adding an addition to an existing structure |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Maintenance and Testing** | Taking a fire alarm system out-of-service |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Taking a sprinkler system out-of-service |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Disconnecting alarm devices |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

 Reviewed Feb 2015